Devices and Modules: Routers

All images on this page are thumbnails on which you can click to bring up a larger image.

Router: 1841

The Cisco 1841 Integrated Services Router provides two fixed 10/100 (100BASE-TX) Ethernet ports, two integrated High-Speed WAN Interface Card (HWIC) slots that are compatible with WAN Interface Card (WICs) and Voice/WAN Interface Cards (VWICs), and one internal Advanced Integration Module (AIM) slot.

Module Name | Thumbnails | Description
HWIC-4ESW |  | The HWIC-4ESW provides 4 switching ports.
WIC-1AM |  | The WIC-1AM card features dual RJ-11 connectors, which are used for basic telephone service connection. The WIC-1AM uses one port for connection to a standard telephone line, and the other port can be connected to a basic analog telephone for use when the modem is idle.
WIC-1ENET |  | The WIC-1ENET is a single-port 10 Mbps Ethernet interface card, for use with 10BASE-T Ethernet LANs.
WIC-1T |  | The WIC-1T provides a single port serial connection to remote sites or legacy serial network devices such as Synchronous Data Link Control (SDLC) concentrators, alarm systems, and packet over SONET (POS) devices.
WIC-2AM |  | The WIC-2AM card features dual RJ-11 connectors, which are used for basic telephone service connection. The WIC-2AM has two modem ports to allow multiple data communication connections.
WIC-2T |  | The 2-port asynchronous/synchronous serial network module provides flexible multi-protocol support, with each port individually configurable in synchronous or asynchronous mode, offering mixed-media dial support in a single chassis. Applications for Asynchronous/Synchronous support include: Low speed WAN aggregation (up to 128 Kbps), dial-up modem support, Async or Sync connections to management ports of other equipment, and transport of legacy protocols such as Bi-sync and SDLC.
WIC-Cover |  | The WIC cover plate provides protection for the internal electronic components. It also helps maintain adequate cooling by normalizing airflow.

Router: 2620XM

The Cisco 2620XM Multiservice Router provides a one-network module slot platform with one fixed 10/100 (100BASE-TX) Ethernet port, two integrated WAN Interface Card (WIC) slots, and one Advanced Integration Module (AIM) slot.

Module Name | Thumbnails | Description
NM-1E |  | The NM-1E features a single Ethernet port that can connect a LAN backbone which can also support either six PRI connections to aggregate ISDN lines, or 24 synchronous/asynchronous ports.
NM-1E2W |  | The NM-1E2W provides a single Ethernet port with two WIC slots that can support a single Ethernet LAN, together with two serial/ISDN backhaul lines, and still allow multiple serial or ISDN in the same chassis.
NM-1FE-FX |  | The NM-1FE-FX Module provides 1 Fast-Ethernet interface for use with fiber media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet.
NM-1FE-TX |  | The NM-1FE-TX Module provides 1 Fast-Ethernet interface for use with copper media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet. The TX (copper) version supports virtual LAN (VLAN) deployment.
NM-1FE2W |  | The NM-1FE2W Module provides 1 Fast-Ethernet interface for use with copper media, in addition to 2 Wan Interface Card expansion slots. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet. The TX (copper) version supports virtual LAN (VLAN) deployment.
NM-2E2W |  | The NM-2E2W provides two Ethernet ports with two WIC slots that can support two Ethernet LANs, together with two serial/ISDN backhaul lines, and still allow multiple serial or ISDN in the same chassis.
NM-2FE2W |  | The NM-2FE2W Module provides 2 Fast-Ethernet interfaces for use with copper media, in addition to 2 Wan Interface Card expansion slots. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards.
NM-2W |  | The NM-2W Module provides 2 Wan Interface Card expansion slots. It can be used with a broad range of interface cards supporting a diverse array of physical media and network protocols.
NM-4A/S |  | The 4-port asynchronous/synchronous serial network module provides flexible multi-protocol support, with each port individually configurable in synchronous or asynchronous mode, offering mixed-media dial support in a single chassis. Applications for Asynchronous/Synchronous support include: Low speed WAN aggregation (up to 128 Kbps), dial-up modem support, Async or Sync connections to management ports of other equipment, and transport of legacy protocols such as Bi-sync and SDLC.
NM-4E |  | The NM-4E features four Ethernet ports for multifunction solutions that require higher-density Ethernet than the mixed-media network modules.
NM-8A/S |  | The 8-port asynchronous/synchronous serial network module provides flexible multi-protocol support, with each port individually configurable in synchronous or asynchronous mode, offering mixed-media dial support in a single chassis. Applications for Asynchronous/Synchronous support include: Low speed WAN aggregation (up to 128 Kbps), dial-up modem support, Async or Sync connections to management ports of other equipment, and transport of legacy protocols such as Bi-sync and SDLC.
NM-8AM |  | The NM-8AM Integrated V.92 analog modem network module provides cost-effective analog telephone service connectivity for lower-density remote-access service (RAS), dial-out and fax-out modem access, asynchronous dial-on-demand routing (DDR) plus dial backup, and remote router management. Both the 8-port and 16-port versions use RJ-11 jacks to connect the integrated modems to basic analog telephone lines on the public switched telephone network (PSTN) or private telephony systems.
NM-Cover |  | The NM cover plate provides protection for the internal electronic components. It also helps maintain adequate cooling by normalizing airflow.
WIC-1AM |  | The WIC-1AM card features dual RJ-11 connectors, which are used for basic telephone service connection. The WIC-1AM uses one port for connection to a standard telephone line, and the other port can be connected to a basic analog telephone for use when the modem is idle.
WIC-1T |  | The WIC-1T provides a single port serial connection to remote sites or legacy serial network devices such as Synchronous Data Link Control (SDLC) concentrators, alarm systems, and packet over SONET (POS) devices.
WIC-2AM |  | The WIC-2AM card features dual RJ-11 connectors, which are used for basic telephone service connection. The WIC-2AM has two modem ports to allow multiple data communication connections.
WIC-2T |  | The 2-port asynchronous/synchronous serial network module provides flexible multi-protocol support, with each port individually configurable in synchronous or asynchronous mode, offering mixed-media dial support in a single chassis. Applications for Asynchronous/Synchronous support include: Low speed WAN aggregation (up to 128 Kbps), dial-up modem support, Async or Sync connections to management ports of other equipment, and transport of legacy protocols such as Bi-sync and SDLC.
WIC-Cover |  | The WIC cover plate provides protection for the internal electronic components. It also helps maintain adequate cooling by normalizing airflow.

Router: 2621XM

The Cisco 2621XM Multiservice Router provides a one-network module slot platform with two fixed 10/100 (100BASE-TX) Ethernet ports, two integrated WAN Interface Card (WIC) slots, and one Advanced Integration Module (AIM) slot.

The 2621XM supports the same modules that the 2620XM supports.

Router: 2811

The Cisco 2811 Integrated Services Router provides one Enhanced Network-Module slot with two fixed 10/100 (100BASE-TX) Ethernet ports, four integrated High-Speed WAN Interface Card (HWIC) slots that are compatible with WAN Interface Card (WICs), Voice Interface Cards (VICs) and Voice/WAN Interface Cards (VWICs), and dual Advanced Integration Module (AIM) slots.

Module Name | Thumbnails | Description
NM-1E |  | The NM-1E features a single Ethernet port that can connect a LAN backbone which can also support either six PRI connections to aggregate ISDN lines, or 24 synchronous/asynchronous ports.
NM-1E2W |  | The NM-1E2W provides a single Ethernet port with two WIC slots that can support a single Ethernet LAN, together with two serial/ISDN backhaul lines, and still allow multiple serial or ISDN in the same chassis.
NM-1FE-FX |  | The NM-1FE-FX Module provides 1 Fast-Ethernet interface for use with fiber media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet.
NM-1FE-TX |  | The NM-1FE-TX Module provides 1 Fast-Ethernet interface for use with copper media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet. The TX (copper) version supports virtual LAN (VLAN) deployment.
NM-1FE2W |  | The NM-1FE2W Module provides 1 Fast-Ethernet interface for use with copper media, in addition to 2 Wan Interface Card expansion slots. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet. The TX (copper) version supports virtual LAN (VLAN) deployment.
NM-2E2W |  | The NM-2E2W provides two Ethernet ports with two WIC slots that can support two Ethernet LANs, together with two serial/ISDN backhaul lines, and still allow multiple serial or ISDN in the same chassis.
NM-2FE2W |  | The NM-2FE2W Module provides 2 Fast-Ethernet interfaces for use with copper media, in addition to 2 Wan Interface Card expansion slots. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards.
NM-2W |  | The NM-2W Module provides 2 Wan Interface Card expansion slots. It can be used with a broad range of interface cards supporting a diverse array of physical media and network protocols.
NM-4A/S |  | The 4-port asynchronous/synchronous serial network module provides flexible multi-protocol support, with each port individually configurable in synchronous or asynchronous mode, offering mixed-media dial support in a single chassis. Applications for Asynchronous/Synchronous support include: Low speed WAN aggregation (up to 128 Kbps), dial-up modem support, Async or Sync connections to management ports of other equipment, and transport of legacy protocols such as Bi-sync and SDLC.
NM-4E |  | The NM-4E features four Ethernet ports for multifunction solutions that require higher-density Ethernet than the mixed-media network modules.
NM-8A/S |  | The 8-port asynchronous/synchronous serial network module provides flexible multi-protocol support, with each port individually configurable in synchronous or asynchronous mode, offering mixed-media dial support in a single chassis. Applications for Asynchronous/Synchronous support include: Low speed WAN aggregation (up to 128 Kbps), dial-up modem support, Async or Sync connections to management ports of other equipment, and transport of legacy protocols such as Bi-sync and SDLC.
NM-8AM |  | The NM-8AM Integrated V.92 analog modem network module provides cost-effective analog telephone service connectivity for lower-density remote-access service (RAS), dial-out and fax-out modem access, asynchronous dial-on-demand routing (DDR) plus dial backup, and remote router management. Both the 8-port and 16-port versions use RJ-11 jacks to connect the integrated modems to basic analog telephone lines on the public switched telephone network (PSTN) or private telephony systems.
NM-Cover |  | The NM cover plate provides protection for the internal electronic components. It also helps maintain adequate cooling by normalizing airflow.
NM-ESW-161 |  | The NM-ESW-161 provides 16 switching ports.
HWIC-4ESW |  | The HWIC-4ESW provides 4 switching ports.
WIC-1AM |  | The WIC-1AM card features dual RJ-11 connectors, which are used for basic telephone service connection. The WIC-1AM uses one port for connection to a standard telephone line, and the other port can be connected to a basic analog telephone for use when the modem is idle.
WIC-1ENET |  | The WIC-1ENET is a single-port 10 Mbps Ethernet interface card, for use with 10BASE-T Ethernet LANs.
WIC-1T |  | The WIC-1T provides a single port serial connection to remote sites or legacy serial network devices such as Synchronous Data Link Control (SDLC) concentrators, alarm systems, and packet over SONET (POS) devices.
WIC-2AM |  | The WIC-2AM card features dual RJ-11 connectors, which are used for basic telephone service connection. The WIC-2AM has two modem ports to allow multiple data communication connections.
WIC-2T |  | The 2-port asynchronous/synchronous serial network module provides flexible multi-protocol support, with each port individually configurable in synchronous or asynchronous mode, offering mixed-media dial support in a single chassis. Applications for Asynchronous/Synchronous support include: Low speed WAN aggregation (up to 128 Kbps), dial-up modem support, Async or Sync connections to management ports of other equipment, and transport of legacy protocols such as Bi-sync and SDLC.
WIC-Cover |  | The WIC cover plate provides protection for the internal electronic components. It also helps maintain adequate cooling by normalizing airflow.

Router: Router-PT

The Router-PT generic router provides ten slots, one console port, and one auxiliary port.

Module Name | Thumbnail | Description
PT-ROUTER-NM-1AM |  | The PT-ROUTER-NM-1AM card features dual RJ-11 connectors, which are used for basic telephone service connection. The WIC-1AM uses one port for connection to a standard telephone line, and the other port can be connected to a basic analog telephone for use when the modem is idle.
PT-ROUTER-NM-1CE |  | The PT-ROUTER-NM-1CE features a single Ethernet port that can connect a LAN backbone which can also support either six PRI connections to aggregate ISDN lines, or 24 synchronous/asynchronous ports.
PT-ROUTER-NM-1CFE |  | The PT-ROUTER-NM-1CFE Module provides 1 Fast-Ethernet interface for use with copper media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet. The TX (copper) version supports virtual LAN (VLAN) deployment.
PT-ROUTER-NM-1CGE |  | The single-port Cisco Gigabit Ethernet Network Module (part number PT-ROUTER-NM-1CGE) provides Gigabit Ethernet copper connectivity for access routers. The module is supported by the Cisco 2691, Cisco 3660, Cisco 3725, and Cisco 3745 series routers. This network module has one gigabit interface converter (GBIC) slot to carry any standard copper or optical Cisco GBIC.
PT-ROUTER-NM-1FFE |  | The PT-ROUTER-NM-1FFE Module provides 1 Fast-Ethernet interface for use with fiber media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet.
PT-ROUTER-NM-1FGE |  | The single-port Cisco Gigabit Ethernet Network Module (part number PT-ROUTER-NM-1FGE) provides Gigabit Ethernet copper connectivity for access routers. The module is supported by the Cisco 2691, Cisco 3660, Cisco 3725, and Cisco 3745 series routers. This network module has one gigabit interface converter (GBIC) slot to carry any standard copper or optical Cisco GBIC.
PT-ROUTER-NM-1S |  | The PT-ROUTER-NM-1S provides a single port serial connection to remote sites or legacy serial network devices such as Synchronous Data Link Control (SDLC) concentrators, alarm systems, and packet over SONET (POS) devices.
PT-ROUTER-NM-1SS |  | The 2-port asynchronous/synchronous serial network module provides flexible multi-protocol support, with each port individually configurable in synchronous or asynchronous mode, offering mixed-media dial support in a single chassis. Applications for Asynchronous/Synchronous support include: Low speed WAN aggregation (up to 128 Kbps), dial-up modem support, Async or Sync connections to management ports of other equipment, and transport of legacy protocols such as Bi-sync and SDLC.