Devices and Modules: End Devices

All images on this page are thumbnails in which you can click to bring up a larger image.

PC-PT

The PC-PT provides a console port and one slot.

Module Name | Thumbnail | Description
Linksys-WMP300N |  | The Linksys-WMP300N module provides one 2.4GHz wireless interface suitable for connection to wireless networks. The module supports protocols that use Ethernet for LAN access.
PC-HOST-NM-1AM |  | The PT-HOST-NM-1AM card features dual RJ-11 connectors, which are used for basic telephone service connection. The WIC-1AM uses one port for connection to a standard telephone line, and the other port can be connected to a basic analog telephone for use when the modem is idle.
PC-HOST-NM-1CE |  | The PT-HOST-NM-1CE features a single Ethernet port that can connect a LAN backbone which can also support either six PRI connections to aggregate ISDN lines, or 24 synchronous/asynchronous ports.
PC-HOST-NM-1CFE |  | The PT-HOST-NM-1CFE Module provides 1 Fast-Ethernet interface for use with copper media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet. The TX (copper) version supports virtual LAN (VLAN) deployment.
PC-HOST-NM-1CGE |  | The single-port Cisco Gigabit Ethernet Network Module (part number PT-HOST-NM-1CGE) provides Gigabit Ethernet copper connectivity for access routers. The module is supported by the Cisco 2691, Cisco 3660, Cisco 3725, and Cisco 3745 series routers. This network module has one gigabit interface converter (GBIC) slot to carry any standard copper or optical Cisco GBIC.
PC-HOST-NM-1FFE |  | The PT-HOST-NM-1FFE Module provides 1 Fast-Ethernet interface for use with fiber media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet.
PC-HOST-NM-1FGE |  | The single-port Cisco Gigabit Ethernet Network Module (part number PT-HOST-NM-1FGE) provides Gigabit Ethernet optical connectivity for access routers. The module is supported by the Cisco 2691, Cisco 3660, Cisco 3725, and Cisco 3745 series routers. This network module has one gigabit interface converter (GBIC) slot to carry any standard copper or optical Cisco GBIC.
PC-HOST-NM-1W |  | The PT-HOST-NM-1W module provides one 2.4GHz wireless interface suitable for connection to wireless networks. The module supports protocols that use Ethernet for LAN access.

Server-PT

The Server-PT provides one slot.

The Server-PT supports the same modules as the PC-PT except for the PC-HOST-NM-1AM module.

Printer-PT

The Printer-PT provides one slot.

The Printer-PT supports the same modules as the PC-PT except for the PC-HOST-NM-1AM module.

IPPhone-PT

The IPPhone-PT does not provide any slots.