Configuring Linksys WRT300N

The Config tab offers two general levels of configuration: global and interface. To configure at the global level, press the GLOBAL button to expand the Settings button (if it has not already been expanded). To configure an interface, press the INTERFACE button to expand the list of interfaces, and then choose the interface.

Global Settings

In the global settings, you can change the Display Name of the Linksys WRT300N.

Internet Interface Configuration

In the Internet settings, you can set the Linksys WRT300N connection type to either automatically obtain IP configurations with DHCP, or you can manually set IP configurations with Static.

LAN Interface Configuration

In the LAN settings, you can set the IP Address and Subnet Mask of the LAN.

Wireless Interface Configuration

In the Wireless settings, you can set the SSID; you can also toggle WEP security mode and then set a Key for WEP authentication.